Back To Index << Back To Templates

# Template Medical Devices

Id | 1.3.6.1.4.1.12559.11.10.1.3.1.3.5 | Effective Date | 2013‑12‑20 Other versions this id: eHDSIMedicalDevice as of 2022‑03‑09 13:27:31 eHDSIMedicalDevice as of 2020‑09‑09 14:16:50 eHDSIMedicalDevice as of 2020‑04‑16 13:07:31 EntryMedicalDevices as of 2019‑04‑09 10:16:28
Status | Retired | Version Label |
Name | EntryMedicalDevices | Display Name | Medical Devices
Description | The medical devices entry content module describes the kind of device that is, or has been used by the patient
Context | Parent nodes of template element with id 1.3.6.1.4.1.12559.11.10.1.3.1.3.5
Classification | CDA Entry Level Template
Open/Closed | Open (other than defined elements are allowed)
Associated with |
Associated with 3 concepts
Id | Name | Dataset
--- | --- | ---
epsos-dataelement-88 | Medical Devices and Implants Description | epSOS Data Set
epsos-dataelement-89 | Device Code | epSOS Data Set
epsos-dataelement-90 | Implant Date | epSOS Data Set
Example |
Example
<supply moodCode="EVN" classCode="SPLY"> <templateId root="1.3.6.1.4.1.12559.11.10.1.3.1.3.5"/> <id root="2.16.840.1.113883.19.811.3"/> <text> <reference value="#DevDescr"/> </text> <effectiveTime value="20070728"/> <participant typeCode="DEV"> <participantRole classCode="MANU"> <id root=""/> <playingDevice classCode="DEV" determinerCode="INSTANCE"> <code code="" codeSystem=""/> </playingDevice> </participantRole> </participant> <!-- ... --> </supply>
| There is an open issue with this item: epsos-issue-239: Modify effectiveTime element for Medical Device template (Feedback needed)
Item | DT | Card | Conf | Description | Label
--- | --- | --- | --- | --- | ---
hl7:supply |  |  | R | The <supply> element shall be present. The moodCode attribute shall be EVN to reflect that a medical device has been provided. |
@classCode | cs | 1 … 1 | F | SPLY
@moodCode | cs | 1 … 1 | F | EVN
hl7:templateId | II | 1 … 1 | R | The template ID indicates that this content module describes a medical device. |
@root | uid | 1 … 1 | F | 1.3.6.1.4.1.12559.11.10.1.3.1.3.5
hl7:id | II | 0 … * | R | This optional element identifies the provision of the device. |
hl7:code | CD | 0 … 1 | R |  |
hl7:text | ED | 0 … 1 | R | The <text> element references the part of the section narrative, which contains the description of the device. |
epsos-dataelement-88 | Medical Devices and Implants Description | epSOS Data Set
hl7:reference | TEL | 1 … 1 | M |  |
@value |  | 1 … 1 | R | Reference pointing to the narrative, typically #{label}-{generated-id}, e.g. #xxx-1
hl7:effectiveTime | TS | 1 … * | R | The <effectiveTime> element denotes the date and time the device was provided to the patient. For an implanted device, that is the date and time of implantation. |
epsos-dataelement-90 | Implant Date | epSOS Data Set
| Example | Time Stamp <effectiveTime value="20070728"/>
hl7:participant |  | 1 … * | R | The device is represented as a participant in the supply structure. The following descriptions apply to the device structure. |
@typeCode | cs | 1 … 1 | F | DEV
| Example | <participant typeCode="DEV"> <participantRole classCode="MANU"> <id root=""/> <playingDevice classCode="DEV" determinerCode="INSTANCE"> <code code="" codeSystem=""/> <!-- ... --> </playingDevice> </participantRole></participant>
hl7:participantRole |  | 1 … 1 | R |  |
@classCode | cs | 1 … 1 | F | MANU
hl7:id |  | 0 … * | R | The device ID is represented by the <id> element of the participant role. This element is optional, as not all device identifiers (serial numbers) may be known to the provider or patient. |
hl7:playingDevice |  | 1 … 1 | R | The <playingDevice> element describes the device instance. The class code shall contain the value of "DEV", and the determiner code shall contain "INSTANCE". |
@classCode | cs | 1 … 1 | F | DEV
@determinerCode | cs | 1 … 1 | F | INSTANCE
hl7:code |  | 1 … 1 | R | The device code describes the type of device (e.g. arm prosthesis, arterial stent). It shall contain codes from the epSOSMedicalDevices value set OID 1.3.6.1.4.1.12559.11.10.1.3.1.42.8. |
epsos-dataelement-89 | Device Code | epSOS Data Set
| CONF |
The value of @code SHALL be drawn from value set 1.3.6.1.4.1.12559.11.10.1.3.1.42.8 eHDSIMedicalDevice (DYNAMIC)